Blog - Liquid-Phase Exfoliation

Page / - last modified by Victor Zhang on 14:26, 15/11/2020

Liquid-Phase Exfoliation

last modified by Victor Zhang

on 14:26, 15/11/2020

Table of Contents

Seems the two ways to produce graphene that can be done in kitchens are tape and Liquid-Phase Exfoliation.

Tape method is very slow, probably can not produce enough to be useful

Liquid-Phase Exfoliation can be done in kitchen, but will need a lot of equipment and safety measures

Source

Exfoliated graphite

Solvent

40% alcholol in water

nmp

90% ethyl acetate 10% methanol (sabesto cleaner)

Posted by Victor Zhang · Permalink