Blog - Liquid-Phase Exfoliation 

Page / - last modified by Victor Zhang on 14:26, 15/11/2020 

Liquid-Phase Exfoliation 
last modified by Victor Zhang
on 14:26, 15/11/2020

Table of Contents

Seems the two ways to produce graphene that can be done in kitchens are tape and Liquid-Phase Exfoliation.
•	Tape method is very slow, probably can not produce enough to be useful
•	Liquid-Phase Exfoliation can be done in kitchen, but will need a lot of equipment and safety measures
•	Source
•	Exfoliated graphite 
•	Solvent
•	40% alcholol in water
•	nmp
•	90% ethyl acetate 10% methanol (sabesto cleaner)
Posted by Victor Zhang  · Permalink