Past works - ESP8266 Docking Board

Page / - last modified by Victor Zhang on 13:54, 09/01/2020

ESP8266 Docking Board

last modified by Victor Zhang

on 13:54, 09/01/2020

Table of Contents

Brief Description:
This is a docking board for NodeMCU 1.0 (ESP-12E), the purpose of the board is for rapid low fidelity prototyping. PIN OUT follows the RC servo standard of [S, V, G] so that most simple modules could be connected with ease. I2C/SPI port also reserved for use for more complex modules. The design does not have a small form factor and does not look optimized because it was designed for versatility. [More ...]